**Note to Designers: Do not use Pay Item 204 Embedment Material measured by the cubic yard for masonry culverts, headwalls and drainage structures other than conduit.**

**SECTION 204**

**STRUCTURE EXCAVATION FOR CONDUIT AND MINOR STRUCTURES**

04/04/18 (N75)

**204-2.01 MATERIALS.** *Delete the first paragraph and substitute the following:*

Embedment Material: Embedment Material consists of bedding, and backfill to 12 inches above the pipe. Use Selected Material, Type A (Subsection 703-2.07) passing the 2-inch sieve for embedment material between vertical planes 18 inches outside the horizontal projection of the outer most diameter of the pipe, horizontal planes located 12 inches above and below the outermost diameter of the pipe or to the depth shown on the Plans.

**204-4.01** **METHOD OF MEASUREMENT.** *Delete the first sentence and substitute the following:* Embedment Material will be measured according to Section 109 as follows:

1. 204.2002.0000 By neat line volume.
2. 204.2003.0000 Will not be measured directly for payment.
3. 204.2004.0000 By weighing.

Structure Excavation will be measured according to Section 109 using neat line method as follows:

**204-5.01 BASIS OF PAYMENT.** *Add the following:* The contract price includes all work and materials necessary to provide, place, and compact Embedment Material.

*Add the following pay items:*

|  |  |
| --- | --- |
| **Pay Item** | **Pay Unit** |
| 204.2002.0000 Embedment Material | Cubic Yard |
| 204.2003.0000 Embedment Material | Lump Sum |
| 204.2004.0000 Embedment Material | Ton |